CGAL 4.7 - 3D Mesh Generation: CGAL::Compact_mesh_cell_base_3< Gt, MD, Tds > Class Template Reference

\( \newcommand{\E}{\mathrm{E}} \) \( \newcommand{\A}{\mathrm{A}} \) \( \newcommand{\R}{\mathrm{R}} \) \( \newcommand{\N}{\mathrm{N}} \) \( \newcommand{\Q}{\mathrm{Q}} \) \( \newcommand{\Z}{\mathrm{Z}} \) \( \def\ccSum #1#2#3{ \sum_{#1}^{#2}{#3} } \def\ccProd #1#2#3{ \sum_{#1}^{#2}{#3} }\)

CGAL 4.7 - 3D Mesh Generation

All Classes Namespaces Files Functions Variables Typedefs Enumerations Enumerator Groups Pages
CGAL::Compact_mesh_cell_base_3< Gt, MD, Tds > Class Template Reference
Mesh Classes

`#include <CGAL/Compact_mesh_cell_base_3.h>`

## Definition

### template<typename Gt, typename MD, typename Tds = void>
class CGAL::Compact_mesh_cell_base_3< Gt, MD, Tds >

The class `Compact_mesh_cell_base_3<Gt, MD>` is a model of the concept `MeshCellBase_3`.

It is designed to serve as cell base class for the 3D triangulation used in the 3D mesh generation process. It is more compact in memory than `Mesh_cell_base_3`.

Template Parameters

  Gt | is the geometric traits class. It has to be a model of the concept `RegularTriangulationTraits_3`.
  MD | provides the types of indices used to identify the faces of the input complex. It has to be a model of the concept `MeshDomain_3`.
  Tds | is the triangulation data structure class to which cells belong. That parameter is only used by the rebind mechanism (see `TriangulationDSCellBase_3::Rebind_TDS`). Users should always use the default parameter value `void`.

Is Model Of:
  `MeshCellBase_3`

See Also
  `CGAL::Mesh_complex_3_in_triangulation_3<Tr,CornerIndex,CurveSegmentIndex>`
  `CGAL::Mesh_cell_base_3<Gt, MD, Cb>`