| Home | Libraries | People | FAQ | More

### Gettable serial port option requirements

In the table below, `X` denotes a serial port option class, `a` denotes a value of `X`, `ec` denotes a value of type `error_code`, and `s` denotes a value of implementation-defined type `storage` (where `storage` is the type `DCB` on Windows and `termios` on POSIX platforms), and `u` denotes an identifier.

Table 11. GettableSerialPortOption requirements

expression | type | assertion/note pre/post-conditions
--- | --- | ---
`const` `storage``& u = s;` `a.load(u, ec);` | `error_code` | Retrieves the value of the serial port option from the storage. If successful, sets `ec` such that `!ec` is true. If an error occurred, sets `ec` such that `!!ec` is true. Returns `ec`.