
namespace CGAL {
/*!

\mainpage User Manual
\anchor Chapter_Advancing_Front_Surface_Reconstruction
\anchor I1ChapterAdvancingFrontSurfaceReconstruction
\cgalAutoToc
\author Tran Kai Frank Da and David Cohen-Steiner

Surface reconstruction from an unstructured point cloud amounts to
generate a plausible surface that approximates well the input
points. This problem is ill-posed as many surfaces can be generated. A
wide range of approaches have been proposed to tackle this
problem. Among them are variational methods
\cgalCite{s-lsm-96}\cgalCite{zomk-insru-00}, tensor voting
\cgalCite{cgal:ml-cfsg-00}, implicit surface
\cgalCite{hddhjmss-pssr-94}\cgalCite{bc-ssrnn-00}, and Delaunay
triangulations.

For Delaunay based algorithms the output surface is commonly generated
as the union of some triangles selected in the 3D Delaunay
triangulation of the input points. Such algorithms are either
volume-based by generating as output the boundary of selected
tetrahedra \cgalCite{abe-cbscc-97}\cgalCite{ack-pcubm-01},
or surface-based by selecting a set of triangles.


In most surface based Delaunay algorithms the triangles are
selected independently, that is in parallel \cgalCite{agj-lcsr-00}\cgalCite{ab-srvf-98}.

This chapter presents a surface-based Delaunay surface
reconstruction algorithm that sequentially selects the triangles, that
is it uses previously selected triangles to select a new triangle for
advancing the front. At each advancing step the most plausible
triangle is selected, and such that the triangles selected
generates an orientable manifold triangulated surface.

Two other examples of this greedy approach are the ball pivoting
algorithm and Boyer-Petitjean's algorithm \cgalCite{bmrst-bpasr-99}\cgalCite{pb-rnrps-01}. In both algorithms
a triangulated surface is incrementally grown starting from a seed
triangle. Ball pivoting is fast, but the quality of the reconstruction
depends on user defined parameters corresponding to the sampling
density. The Boyer-Petitjean approach can handle non-uniform sampling,
but fails when near co-circular points are encountered, and it does
not provide any guarantee on the topology of the surface.

We describe next the algorithm and provide examples.


\section AFSR_Definitions Definitions and the Algorithm

A detailed description of the algorithm and the underlying theory are provided
in \cgalCite{cgal:csd-gdbsra-04}.

The first step of the algorithm is the construction of a 3D Delaunay
triangulation of the point set.
The radius of a triangle \f$ t \f$ is the radius of the smallest sphere
passing through the vertices of \f$ t\f$ and enclosing no sample
point. In other words, the radius \f$ r_t\f$ is the distance from any
vertex of \f$ t\f$ to the Voronoi edge dual to \f$ t\f$. This triangle with
three boundary edges is the initial triangulated surface, and its
boundary is the advancing front.
The Delaunay triangle with the smallest radius is the starting point
for the greedy algorithm.

The algorithm maintains a priority queue of candidate triangles, that
is of valid triangles incident to the boundary edges of the current
surface. The priority is the plausibility. While the priority queue is
not empty, the algorithm pops from the queue the most plausible
candidate triangle and adds it to the surface. New candidate triangles
are pushed to the priority queue when new boundary edges appear on the
advancing front. As the algorithm creates a two-manifold surface some
candidate triangles can not be selected due to topological constraints
which are explained next.


\subsection AFSR_Topology Topological Constraints

Any triangle \f$t\f$ considered as the next potential candidate shares an
edge \f$e\f$ with the front of the current reconstruction. Let \f$b\f$
be the vertex of \f$t\f$ opposite to \f$e\f$. There are four
configurations where \f$t\f$ is added to the surface.

- extension,  if \f$b\f$ is not yet on the surface.
- hole filling, if \f$b\f$ is on the front and both neighbors of \f$b\f$ on the front are on edge \f$e\f$.
- ear filling, if \f$b\f$ is on the front and one neighbor of \f$b\f$ on the front is on edge \f$e\f$.
- glueing, if \f$b\f$ is on the front and no neighbor of \f$b\f$ on the front is on edge \f$e\f$.

\cgalFigureBegin{figAFSRvalid,valid.png}
Valid candidates.
\cgalFigureEnd

While the first three operations never induce a non-manifold edge or vertex,
we only can perform gluing, if triangle \f$t\f$ has a *twin* facet, that is a
triangle with an edge on the front and incident to \f$b\f$, and the
third vertex on edge \f$e\f$.

A triangle is said  *valid* when the above operations can be applied.

\subsection AFSR_Selection Plausibility of a Candidate Triangle

Valid triangles for an edge on the front are compared through their
radius. While the radius is a good criterion in the case of 2D smooth
curve reconstruction \cgalCite{b-cccda-94}, we need another criterion
for 3D surface reconstruction, namely the dihedral angle between
triangles on the surface, that is the angle between the normals of the
triangles. There are three bounds namely \f$ \alpha_\mathrm{sliver} \f$,
\f$ \beta \f$, and \f$ \delta \f$.

The *candidate* triangle of an edge \f$ e \f$ is the triangle
with the smallest radius:
- that is valid for \f$ e \f$, and
- that has \f$ \beta_t < \alpha_\mathrm{sliver} \f$, and
- that has its internal angles with \f$ e \f$ smaller than \f$ \delta \f$.

There may be no such triangle. In the implementation
of the algorithm \f$ \alpha_\mathrm{sliver} \f$ and \f$ \delta\f$ are equal
to \f$ 5\pi/6 \f$.


We denote by \f$ \beta_t\f$ the angle between the normal of a triangle
\f$ t\f$ incident on a boundary edge \f$ e \f$ and the normal of the
triangle on the surface incident to \f$ e \f$.


We define the *plausibility* grade \f$ p(t) \f$ as \f$ 1/r_t \f$, if
\f$ \beta_t < \beta \f$, and \f$ -\beta_t \f$ else.  The parameter \f$
\beta \f$ can be specified by the user and is set by default to \f$ \pi/6\f$.

Let's have a look at the figure below.
\cgalFigureBegin{figAFSRplausible,wedges.png}
Plausibility. Triangle `t'` and incidident triangles sharing edge `e` seen from the side.
\cgalFigureEnd

 \f$ \alpha_\mathrm{sliver}\f$ corresponds to the red wedge. The algorithm will never select triangle `t1`
even if it is the only candidate triangle.

\f$\beta\f$ corresponds to the green wedge. If there is a candidate triangle in this zone,
the one with the smallest radius is the most plausible.

If there is no candidate triangle in the green wedge, the triangle with the smallest
angle between its normal and the normal of `t'` is chosen.  In the figure above
this would be triangle `t4`.

\subsection AFSR_Boundaries Dealing with Multiple Components, Boundaries and Sharp Edges

By construction the output of the algorithm is a connected orientable
manifold with or without boundary. To cope with multiple components we
merely look for a new seed facet among facets disjoint from the
surface. In case of noisy data or outliers, the user must filter out
small surface components.

It is impossible to handle all kinds of boundaries and non uniform sampling
at the same time, as a void can either be an undersampled area of the surface,
or a hole.

As we do not want the algorithm to rely on a uniformity condition on
the sampling it will fill holes cut off from "flat" regions of the
surface. However, in many cases a boundary component cannot be closed
by adding a spanning disk such that the resulting disk is well
sampled. Typically, closing a boundary component due to a transversal
clipping of the operation, would yield large dihedral angles at
boundary edges. Moreover, if the boundary is sufficiently well
sampled, the radii of the two triangles incident on a boundary edge
would be very different.  These heuristic facts can be used for
boundary detection.

More specifically, we discard any candidate triangle \f$ t \f$, for an edge \f$ e \f$
such that \f$ p(t) < 0\f$, and \f$ r_t > \mathrm{radius\_ratio\_bound} \times r_{t'}\f$ where \f$ t'\f$ is
the triangle on the surface incident on \f$ e \f$. The parameter \f$\mathrm{radius\_ratio\_bound}\f$
is specified by the user and is set by default to 5.

For the example given in  \cgalFigureRef{figAFSRplausible}, we said that if there
was no triangle `t3` in the green wedge, triangle `t4` would be chosen as it has
the smallest angle between its normal and the normal of triangle `t'`.
However, in case its radius was \f$\mathrm{radius\_ratio\_bound}\f$ times larger than the radius of triangle `t'`,
triangle `t2` would be chosen, assuming that its radius is not  \f$\mathrm{radius\_ratio\_bound}\f$ times larger.


Note that this heuristic implies that
where the sampling is too sparse with respect to curvature, it must
be sufficiently uniform for our algorithm to work.


\section AFSR_Examples Examples

The first of the following three examples presents a free function for doing surface
reconstruction. For a sequence of points the function produces a sequence
of triplets of indices describing the triangles of the surface.
The second example presents a class that enables to traverse the
surface represented in a 2D triangulation data structure where
the faces are connected with the facets of underlying 3D Delaunay triangulation.
The third example shows how to get outliers and the boundaries of
the surface. The last example shows how to combine this algorithm with
two \cgal algorithms in order to reconstruct surfaces with sharp
features.

\subsection AFSR_Example_function Examples for Global Function

The global function `advancing_front_surface_reconstruction()`
takes an iterator range of points as input and writes for each face of the
reconstructed surface a triplet of point indices into an output iterator.
The following example writes the output triangulated surface to `std::cout`
in accordance to the OFF format.

The function has an overload with an additional argument that allows
to choose how to prioritize facets. It can be written in a way to
avoid the generation of triangles with a perimeter larger than a given
bound.

\cgalExample{Advancing_front_surface_reconstruction/reconstruction_fct.cpp}


While the first example just writes index triples, the second example
uses as output iterator a wrapper around a reference to a `Surface_mesh`
and calls the function `add_face()`.

\cgalExample{Advancing_front_surface_reconstruction/reconstruction_surface_mesh.cpp}


\subsection AFSR_Example_class Example for the Reconstruction Class

The class `Advancing_front_surface_reconstruction` provides
access to a 2D triangulation data structure describing the output surface.
The latter can be explored by hopping from a face to its neighboring faces,
and by hopping from faces of the 2D triangulation data structure to
corresponding facets of the underlying 3D Delaunay triangulation.

The type of the 2D triangulation data structure describing the
reconstructed surface is the nested type
\link Advancing_front_surface_reconstruction::Triangulation_data_structure_2 `Advancing_front_surface_reconstruction::Triangulation_data_structure_2`\endlink.

The type `Advancing_front_surface_reconstruction::Triangulation_data_structure_2::Vertex` is model of the
concept `TriangulationDataStructure_2::Vertex` and has additionally
the method `vertex_3()` that returns an `Advancing_front_surface_reconstruction::Vertex_handle` to the
associated 3D vertex.

 The type `Advancing_front_surface_reconstruction::Triangulation_data_structure_2::Face` is model of the concept
`TriangulationDataStructure_2::Face` and has additionally the method
`facet()` that returns the associated `Advancing_front_surface_reconstruction::Facet`,
and a method `is_on_surface()` for testing if a face is part of the reconstructed
surface.

In case the surface
has boundaries, the 2D surface has one vertex which is associated to
the infinite vertex of the 3D triangulation.


The underlying 3D Delaunay triangulation can be accessed as well,
using the API of the class `Delaunay_triangulation_3`.

The following example writes the surface to `std::cout` in accordance
to the STL (Stereo Lithography) format.

\cgalExample{Advancing_front_surface_reconstruction/reconstruction_class.cpp}


\subsection AFSR_Example_boundaries Example for Outliers and Boundaries

Input points which are not on
a surface are outliers. The member function \link Advancing_front_surface_reconstruction::outliers() `outliers()`\endlink
returns an iterator range of those points.

Boundary edges can be traversed with the member function \link Advancing_front_surface_reconstruction::boundaries() `boundaries()`\endlink
It returns an iterator range type \link Advancing_front_surface_reconstruction::Boundary_range `Boundary_range`\endlink whose iterators have the value type
\link Advancing_front_surface_reconstruction::Vertex_on_boundary_range `Vertex_on_boundary_range`\endlink.  This is again an iterator range whose iterators have the value type
\link Advancing_front_surface_reconstruction::Vertex_handle `Vertex_handle`\endlink.

\cgalExample{Advancing_front_surface_reconstruction/boundaries.cpp}

\subsection AFSR_Example_sharp_features Example for Sharp Features

The priority queue used by the advancing front surface reconstruction
algorithm can be modified to achieve robustness to sharp edges and
provide piecewise-planar or hybrid reconstruction as described in
\cgalCite{cgal:la-srpss-13}. Two other algorithms available in \cgal
must be applied first as a preprocessing to the point set:

- \ref Chapter_Point_Set_Shape_Detection "Shape detection": detect planar sections of the input.

- \ref Point_set_processing_3Structuring "Point set structuring":
resample the planar sections and edges and corners detected among
them.

\cgalFigureBegin{figAFSRstruct,structured_example.png}
Comparison of advancing front output.

- Top: input point set and raw advancing front reconstruction

- Bottom: structured point set and advancing front reconstruction with
structure-dependent priority functor

\cgalFigureEnd

The quality of the reconstruction can be significantly improved thanks
to point set structuring when dealing with shapes with sharp features,
as shown on the previous figure. The following example shows how to
define a priority functor that favors structurally coherent facets and
makes the advancing front algorithm robust to sharp features.


\cgalExample{Advancing_front_surface_reconstruction/reconstruction_structured.cpp}





*/
} /* namespace CGAL */

